Current configuration : 1851 bytes

Last configuration change at 11:50:26 UTC Wed Jan 31 2024

NVRAM config last updated at 11:51:58 UTC Wed Jan 31 2024

version 12.2

no service pad

service timestamps debug datetime msec

service timestamps log datetime msec

service password-encryption

hostname B513-Cisco2960-08

boot-start-marker

boot-end-marker

enable secret 5 $1$L4mo$bmu5GpQwi0EoQnXkPCCX21

enable password 7 106C1D5D41561D

username btssio password 7 04591F151C2843

no aaa new-model

system mtu routing 1500

--More--

ip domain-name 0870019y.lan

spanning-tree mode pvst

spanning-tree extend system-id

vlan internal allocation policy ascending

ip ssh time-out 50

ip ssh authentication-retries 5

ip ssh version 1

interface FastEthernet0/1

switchport access vlan 301

switchport mode access

--More-- interface FastEthernet0/2

switchport access vlan 317

switchport mode access

interface FastEthernet0/3

switchport access vlan 314

switchport mode access

interface FastEthernet0/4

switchport access vlan 318

switchport mode access

interface FastEthernet0/5

switchport access vlan 319

switchport mode access

interface FastEthernet0/6

switchport access vlan 352

switchport mode access

interface FastEthernet0/7

switchport access vlan 134

switchport mode access

--More-- interface FastEthernet0/8

switchport mode access

interface GigabitEthernet0/1

switchport mode trunk

interface Vlan1

ip address 10.0.0.254 255.255.255.0

no ip route-cache

interface Vlan134

ip address 10.187.35.28 255.255.255.0

no ip route-cache

ip http server

ip http secure-server

logging esm config

banner motd ^CAcces autoise pour les etudiants et enseignants du BTS SIO seulement

line con 0

password 7 03147B4F42182E5E4A51

login

line vty 0 4

--More-- password 7 104C1D0A161E1D

logging synchronous

login local

transport input telnet ssh

line vty 5 15

login

end

B513-Cisco2960-08#exit